1 CYLINDER, 9/32" BRASS TUBE

2 CYLINDER HEAD, FREE CUTTING BRASS ROD

3 VALVE TUBE, 1/8" BRASS TUBE

4 BRASS TOP, 0.03" x 1/2" BRASS FLAT BAR

5 BRASS BASE, 0.03" x 3/4" BRASS FLAT BAR

6 FRAME POST, 3/32" FREE CUTTING BRASS ROD

7 INLET MANIFOLD, 3/32" BRASS TUBE

8 FLYWHEEL, 1/2" FREE CUTTING BRASS ROD

9 CRANKSHAFT, 5/64" & 3/8" DRILL ROD

10 0-80 STAINLESS HEX HEAD AND PHILLIPS HEAD BOLTS

11 PISTON, FREE CUTTING BRASS ROD, MACHINE TO FIT

12 VALVE, FREE CUTTING BRASS ROD, MACHINE TO FIT

13 CONNECTING ROD, 1/32" x 3/32" BRASS FLAT BAR

14 MAIN BEARING, FREE CUTTING BRASS ROD

15 VALVE ROD, 1/32" BRASS ROD

16 ECCENTRIC, 1/4" FREE CUTTING BRASS ROD